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LITHIUM BATTERY
28V |8 Ah | 102.4 wh
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CHARGE SPECIFICATIONS�
�
Recommended Charge Current�
1.6 A�
�
Maximum Charge Current�
8 A�
�
Recommended Charge Voltage�
14.2 V – 14.6V�
�



BMS Charge Voltage Cut-Off�
15.0 V (3.75 ±0.025 v) (2 s)�
�
Reconnect Voltage�
14.0 V (3.5 ±0.05 v)�
�
Balancing Voltage�
13.6 V (3.4 ±0.025 v)�
�



COMPLIANCE SPECIFICATIONS�
�



Certifications�
UN38.3/CE/


 FCC/ROHS�
�
Shipping Classification�
UN 3480, CLASS 9�
�



DIMENSIONAL SPECIFICATIONS�
�
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�
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ELECTRICAL SPECIFICATIONS�
�
Nominal Voltage�
12.8V�
�
Nominal Capacity�
8 Ah�
�
Capacity @ 1.6A�
300 min�
�



Resistance�



≤65 mΩ @ 50% SOC�
�
Efficiency�
99%�
�
Self Discharge�
<3% per Month�
�
Cycle Life�
2000 times DOD100% (0.5C)�
�
Maximum Modules in Series�
4�
�



DISCHARGE SPECIFICATIONS�
�
Maximum Continuous Discharge Current�
8 A�
�
Peak Discharge Current�
14 A (10-15 s)�
�
BMS Discharge Current Cut-Off�
14 A (10-15 s)�
�
Recommended Low Voltage Disconnect�
11 V�
�
BMS Discharge Voltage Cut-Off�
8.8 V (2.2 ±0.08 v) (2s)�
�
Reconnect Voltage�
10.8 V (2.7 ±0.1 v)�
�
Short Circuit Protection�
200-600 µs�
�



TEMPERATURE SPECIFICATIONS�
�
Discharge Temperature�
-4 to 140 °F (-20 to 60 °C)�
�
Charge Temperature�
32 to 131 °F (0 to 55 °C)�
�
Storage Temperature�
14 to 113 °F (-10 to 45°C)�
�
BMS High Temperature Cut-Off�
167 °F (75 ºC)�
�
Reconnect Temperature�
122°F (50 ºC)�
�



MECHANICAL SPECIFICATIONS�
�



Dimensions (L x W x H)�
5.94 x 2.55 x 3.74 inch


151 x 65 x 95 mm�
�
Weight�
2.6 lbs (1.2 kg)�
�
Terminal Type�
T1�
�
Terminal Torque�
N/A�
�
Case Material�
ABS�
�
Enclosure Protection�
IP65�
�
Cell Type�
LiFePO4�
�

















































































